IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
File name: "91017457-Z07-Anker"
Time stamp: "2024-11-11T16:02:28+06:00"
Author: "rsach"
Preprocessor: "ST-DEVELOPER v16.5"
Originating system: "HiCAD 2024 29.0.1.245"
Application: "HiCAD 2024" version "29.0.1.245" identifier "HiCAD" by Organization "ISD Software und Systeme GmbH"

People and organizations
  Person "rsach" of Organization (no name given)
  Owner history of Person "rsach" of Organization (no name given) | application "HiCAD 2024" version "29.0.1.245" identifier "HiCAD" by Organization "ISD Software und Systeme GmbH" | created 1731321148 (2024-11-11T10:32:28Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "91017457-Z07-ANKER"
  IFCBUILDING "91017457-Z07-ANKER"
    contains 1 element
      1 x IFCBUILDINGELEMENTPROXY | names: "Plaatwerk D= 8mm" | material: "S355J2G3" | property sets: HiCAD_Attributes, HiCAD_InternalData

Property sets
  HiCAD_Attributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    #IP = 1 (IFCINTEGER)
    #SR = 1 (IFCINTEGER)
    $02 = "1x Plaatwerk D= 8mmx242.000x60.000" (IFCTEXT)
    $05 = "Sheet Metal" (IFCTEXT)
    $07 = "S355J2G3" (IFCTEXT)
    $08 = "1.0577" (IFCTEXT)
    $BB = "Plaatwerk D= 8mm" (IFCTEXT)
    $CompDrwName = "800619224" (IFCTEXT)
    $DSTV_N = "" (IFCTEXT)
    $DSTV_T = "H" (IFCTEXT)
    $TN = "800617427" (IFCTEXT)
    %01 = 1 (IFCINTEGER)
    %02 = 100 (IFCINTEGER)
    %06 = 1 (IFCINTEGER)
    %10 = 33 (IFCINTEGER)
    %13 = 1 (IFCINTEGER)
    %PIDX = 1 (IFCINTEGER)
    %VS_ID = 800619223 (IFCINTEGER)
    ITEMID = 20 (IFCINTEGER)
    TABLEID = 335700820 (IFCINTEGER)
    ~vICN = "Plaatwerk D= 8mm {S355J2G3} {} {} {100}" (IFCTEXT)
    §01 = 1.0209343889565 (IFCREAL)
    §02 = 60. (IFCREAL)
    §03 = 242. (IFCREAL)
    §04 = 68. (IFCREAL)
    §10 = 0.0365474686492374 (IFCREAL)
    §20 = 130055.336172803 (IFCREAL)
    §21 = 7.85 (IFCREAL)
    §B2D = 60. (IFCREAL)
    §CW = 1.08018221963475 (IFCREAL)
    §L2D = 286.672563597334 (IFCREAL)
    §S2D = 0.01720035381584 (IFCREAL)
    §SC = 0. (IFCREAL)
    §SOC = 0.01720035381584 (IFCREAL)
    §T2D = 8. (IFCREAL)
  HiCAD_InternalData | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    ExportVersion = "29.0.1.245" (IFCTEXT)
    NodeTypeId: PartType = 3 (IFCINTEGER); Steel = 33 (IFCINTEGER); Special = 30 (IFCINTEGER); Profile = 0 (IFCINTEGER)